,Weight Product##OTHER##,URL##OTHER##,Type##OTHER##,Trim##OTHER##,Transformer Taps##OTHER##,Sensitivity##OTHER##,SPL Max##OTHER##,Rotation##ANGLE##DEGREES,Recommended Tap Selection##ELECTRICAL_WATTAGE##WATTS,Recommended High-Pass Filter##OTHER##,Recommended Amplifier##OTHER##,Rated Power##OTHER##,REP##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Pitch Constraint##ANGLE##DEGREES,Pitch##ANGLE##DEGREES,Peak Factor##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Add Weatherized Connector Cover##OTHER##,40-55 Ceiling Bracket White##OTHER##,40 50 Loudspeaker Rotation##ANGLE##DEGREES,Kit Cover Constraint##OTHER##,Impedance##OTHER##,Horizontal Orientation##OTHER##,Hardware Finish##OTHER##,Grille##OTHER##,Grill Scrim##OTHER##,Grill Finish##OTHER##,Frequency Response##OTHER##,Fittings##OTHER##,Finish##OTHER##,Enclosure##OTHER##,Drivers##OTHER##,Dimensions##OTHER##,Dispersion (-6dB)##OTHER##,Desired Level @ Listener##OTHER##,Description##OTHER##,Default Elevation##LENGTH##FEET,D2##LENGTH##FEET,Crossover##OTHER##,Connectors##OTHER##,Cone Finish##OTHER##,Ceiling Rotation Offset##LENGTH##FEET,Ceiling Mounted##OTHER##,Ceiling Mount Rotation##ANGLE##DEGREES,80 Rotation##ANGLE##DEGREES,80 Ceiling Bracket White##OTHER##,80 Ceiling Bracket Black##OTHER##,Case Finish##OTHER##,Azimuth Constraint##ANGLE##DEGREES,Azimuth##ANGLE##DEGREES,Assembly Code##OTHER##,Accessories (included)##OTHER##,A80T White##OTHER##,A80T Black##OTHER##,A55 White##OTHER##,A55 Black##OTHER##,A40-55 Bracket##OTHER##,A40 White##OTHER##,A40 Black##OTHER##,80 Weather Kit Cover Constraint##OTHER##,80 Azimuth Constraint##ANGLE##DEGREES,55 White Kit Cover Constraint##OTHER##,55 Black Kit Cover Constraint##OTHER##,50 Pitch Constraint##ANGLE##DEGREES,60W XFRM##ELECTRICAL_WATTAGE##WATTS,40-55 Ceiling Bracket Black##OTHER##,40 White Kit Cover Constraint##OTHER##,40 Black Kit Cover Constraint##OTHER##,30W XFRM##ELECTRICAL_WATTAGE##WATTS,100V Circuit Voltage##OTHER##
A40 - Black,3.9,https://martin-audio.com/,"Ultra-compact passive two-way system, front ported bass reflex",Steel - Black Powder coated,N/A,87,109,0.000000000000,10,60Hz 24dB/oct,VIA2004 (for low-impedance operation),"40W AES, 160W peak",8.445563,https://martin-audio.com/products/loudspeakers/a40,https://martin-audio.com/downloads/datasheets/ADORN-A40-datasheet.pdf,90.000000000000,0.000000000000,10,A40 - Black,Martin Audio,0,0,90.000000000000,0,16,0,Steel - Black Powder coated,Perforated steel,"Laminate, Black, Matte",Black Grille,"98Hz-17kHz ± 3dB, -10dB @ 70Hz",Wall bracket included,Black or white,"ABS, UL 94V-0 rated","LF: 4” /1” high-temp voice coil, coated paper cone, rubber surround, ferrite motor, pressed steel chassis. HF: 0.75” silk dome, neodymium motor","(W) 124mm x (H) 200mm x (D) 114mm, (W) 4.9in x (H) 7.9in x (D) 4.5in",110° H x 80° V,75,Ultra-Compact Two-Way On-Wall System,4.000000000000,12.000000000000,3.5 kHz passive (LF and HF auto-resetting fuses),Push terminals,"Rubber, Natural",0.250000000000,0,0.000000000000,90.000000000000,0,0,Black Finish,90.000000000000,0.000000000000,D5030100,Waterproof connector cover,0,0,0,0,1,0,1,0,0.000000000000,0,0,0.000000000000,15,0,0,0,10,0
A40T - Black,3.9,https://martin-audio.com/,"Ultra-compact passive two-way system, front ported bass reflex",Steel - Black Powder coated,"70V:   20w / 10w / 5w / 2.5w, 100V: 20w / 10w / 5w",87,109,0.000000000000,10,60Hz 24dB/oct,VIA2004 (for low-impedance operation),"40W AES, 160W peak",8.445563,https://martin-audio.com/products/loudspeakers/a40t,https://martin-audio.com/downloads/datasheets/ADORN-A40T-datasheet.pdf,90.000000000000,0.000000000000,10,A40T - Black,Martin Audio,0,0,90.000000000000,0,16,0,Steel - Black Powder coated,Perforated steel,"Laminate, Black, Matte",Black Grille,"98Hz-17kHz ± 3dB, -10dB @ 70Hz",Wall bracket included,Black or white,"ABS, UL 94V-0 rated","LF: 4” /1” high-temp voice coil, coated paper cone, rubber surround, ferrite motor, pressed steel chassis. HF: 0.75” silk dome, neodymium motor","(W) 124mm x (H) 200mm x (D) 114mm, (W) 4.9in x (H) 7.9in x (D) 4.5in",110° H x 80° V,75,Ultra-Compact Two-Way On-Wall System - Transformer,4.000000000000,12.000000000000,3.5 kHz passive (LF and HF auto-resetting fuses),Push terminals,"Rubber, Natural",0.250000000000,0,0.000000000000,90.000000000000,0,0,Black Finish,90.000000000000,0.000000000000,D5030100,Waterproof connector cover,0,0,0,0,1,0,1,0,0.000000000000,0,0,0.000000000000,15,0,0,0,10,0
A55 - Black,4.9,https://martin-audio.com/,"Ultra-compact passive two-way system, front ported bass reflex",Steel - Black Powder coated,N/A,90,113,0.000000000000,20,60Hz 24dB/oct,VIA2004 (for low-impedance operation),"50W AES, 200W peak",11.757801,https://martin-audio.com/products/loudspeakers/a55,https://martin-audio.com/downloads/datasheets/ADORN-A55-datasheet.pdf,90.000000000000,0.000000000000,10,A55 - Black,Martin Audio,0,0,90.000000000000,0,16,0,Steel - Black Powder coated,Perforated steel,"Laminate, Black, Matte",Black Grille,"90Hz-17kHz ± 3dB, -10dB @ 65Hz",Wall bracket included,Black or white,"ABS, UL 94V-0 rated","LF: 5.25” /1” high-temp voice coil, coated paper, cone, rubber surround, ferrite motor, pressed steel chassis, HF: 0.75” silk dome, neodymium motor","(W) 152mm x (H) 245mm x (D) 140mm, (W) 6in x (H) 9.6in x (D) 5.5in",110° H x 80° V,75,Ultra-Compact Two-Way On-Wall System,4.000000000000,20.000000000000,3.5 kHz passive (LF and HF auto-resetting fuses),Push terminals,"Rubber, Natural",0.260416666667,0,0.000000000000,90.000000000000,0,0,Black Finish,90.000000000000,0.000000000000,D5030100,Waterproof connector cover,0,0,0,1,1,0,0,0,0.000000000000,0,0,0.000000000000,15,0,0,0,20,0
A40T - White,3.9,https://martin-audio.com/,"Ultra-compact passive two-way system, front ported bass reflex",Steel - White Powder coated,"70V:   20w / 10w / 5w / 2.5w, 100V: 20w / 10w / 5w",87,109,0.000000000000,10,60Hz 24dB/oct,VIA2004 (for low-impedance operation),"40W AES, 160W peak",8.445563,https://martin-audio.com/products/loudspeakers/a40t,https://martin-audio.com/downloads/datasheets/ADORN-A40T-datasheet.pdf,90.000000000000,0.000000000000,10,A40T - White,Martin Audio,0,0,90.000000000000,0,16,0,Steel - White Powder coated,Perforated steel,"Laminate, White, Matte",White Grille,"98Hz-17kHz ± 3dB, -10dB @ 70Hz",Wall bracket included,Black or white,"ABS, UL 94V-0 rated","LF: 4” /1” high-temp voice coil, coated paper cone, rubber surround, ferrite motor, pressed steel chassis. HF: 0.75” silk dome, neodymium motor","(W) 124mm x (H) 200mm x (D) 114mm, (W) 4.9in x (H) 7.9in x (D) 4.5in",110° H x 80° V,75,Ultra-Compact Two-Way On-Wall System - Transformer,4.000000000000,12.000000000000,3.5 kHz passive (LF and HF auto-resetting fuses),Push terminals,"Rubber, Natural",0.250000000000,0,0.000000000000,90.000000000000,0,0,Wear Resistant Textured White,90.000000000000,0.000000000000,D5030100,Waterproof connector cover,0,0,0,0,1,1,0,0,0.000000000000,0,0,0.000000000000,15,0,0,0,10,0
A40 - White,3.9,https://martin-audio.com/,"Ultra-compact passive two-way system, front ported bass reflex",Steel - White Powder coated,N/A,87,109,0.000000000000,10,60Hz 24dB/oct,VIA2004 (for low-impedance operation),"40W AES, 160W peak",8.445563,https://martin-audio.com/products/loudspeakers/a40,https://martin-audio.com/downloads/datasheets/ADORN-A40-datasheet.pdf,90.000000000000,0.000000000000,10,A40 - White,Martin Audio,0,0,90.000000000000,0,16,0,Steel - White Powder coated,Perforated steel,"Laminate, White, Matte",White Grille,"98Hz-17kHz ± 3dB, -10dB @ 70Hz",Wall bracket included,Black or white,"ABS, UL 94V-0 rated","LF: 4” /1” high-temp voice coil, coated paper cone, rubber surround, ferrite motor, pressed steel chassis. HF: 0.75” silk dome, neodymium motor","(W) 124mm x (H) 200mm x (D) 114mm, (W) 4.9in x (H) 7.9in x (D) 4.5in",110° H x 80° V,75,Ultra-Compact Two-Way On-Wall System,4.000000000000,12.000000000000,3.5 kHz passive (LF and HF auto-resetting fuses),Push terminals,"Rubber, Natural",0.250000000000,0,0.000000000000,90.000000000000,0,0,Wear Resistant Textured White,90.000000000000,0.000000000000,D5030100,Waterproof connector cover,0,0,0,0,1,1,0,0,0.000000000000,0,0,0.000000000000,15,0,0,0,10,0
A55 - White,4.9,https://martin-audio.com/,"Ultra-compact passive two-way system, front ported bass reflex",Steel - White Powder coated,N/A,90,113,0.000000000000,5,60Hz 24dB/oct,VIA2004 (for low-impedance operation),"50W AES, 200W peak",4.232808,https://martin-audio.com/products/loudspeakers/a55,https://martin-audio.com/downloads/datasheets/ADORN-A55-datasheet.pdf,90.000000000000,0.000000000000,10,A55 - White,Martin Audio,0,0,90.000000000000,0,16,0,Steel - White Powder coated,Perforated steel,"Laminate, White, Matte",White Grille,"90Hz-17kHz ± 3dB, -10dB @ 65Hz",Wall bracket included,Black or white,"ABS, UL 94V-0 rated","LF: 5.25” /1” high-temp voice coil, coated paper, cone, rubber surround, ferrite motor, pressed steel chassis, HF: 0.75” silk dome, neodymium motor","(W) 152mm x (H) 245mm x (D) 140mm, (W) 6in x (H) 9.6in x (D) 5.5in",110° H x 80° V,75,Ultra-Compact Two-Way On-Wall System,4.000000000000,12.000000000000,3.5 kHz passive (LF and HF auto-resetting fuses),Push terminals,"Rubber, Natural",0.260416666667,0,0.000000000000,90.000000000000,0,0,White Powder Coated Finish,90.000000000000,0.000000000000,D5030100,Waterproof connector cover,0,0,1,0,1,0,0,0,0.000000000000,0,0,0.000000000000,7.5,0,0,0,5,0
A55T - Black,4.9,https://martin-audio.com/,"Ultra-compact passive two-way system, front ported bass reflex",Steel - Black Powder coated,"70V:   30w / 15w / 7.5w / 3.75w, 100V:  30w / 15w / 7.5w",90,113,0.000000000000,5,60Hz 24dB/oct,VIA2004 (for low-impedance operation),"50W AES, 200W peak",4.232808,https://martin-audio.com/products/loudspeakers/a55t,https://martin-audio.com/downloads/datasheets/ADORN-A55T-datasheet.pdf,90.000000000000,0.000000000000,10,A55T - Black,Martin Audio,0,0,90.000000000000,0,16,0,Steel - Black Powder coated,Perforated steel,"Laminate, Black, Matte",Black Grille,"90Hz-17kHz ± 3dB, -10dB @ 65Hz",Wall bracket included,Black or white,"ABS, UL 94V-0 rated","LF: 5.25” /1” high-temp voice coil, coated paper, cone, rubber surround, ferrite motor, pressed steel chassis, HF: 0.75” silk dome, neodymium motor","(W) 152mm x (H) 245mm x (D) 140mm, (W) 6in x (H) 9.6in x (D) 5.5in",110° H x 80° V,75,Ultra-Compact Two-Way On-Wall System - Transformer,4.000000000000,12.000000000000,3.5 kHz passive (LF and HF auto-resetting fuses),Push terminals,"Rubber, Natural",0.260416666667,0,0.000000000000,90.000000000000,0,0,Black Finish,90.000000000000,0.000000000000,D5030100,Waterproof connector cover,0,0,0,1,1,0,0,0,0.000000000000,0,0,0.000000000000,7.5,0,0,0,5,0
A55T - White,4.9,https://martin-audio.com/,"Ultra-compact passive two-way system, front ported bass reflex",Steel - White Powder coated,"70V:   30w / 15w / 7.5w / 3.75w, 100V:  30w / 15w / 7.5w",90,113,0.000000000000,5,60Hz 24dB/oct,VIA2004 (for low-impedance operation),"50W AES, 200W peak",4.232808,https://martin-audio.com/products/loudspeakers/a55t,https://martin-audio.com/downloads/datasheets/ADORN-A55T-datasheet.pdf,90.000000000000,0.000000000000,10,A55T - White,Martin Audio,0,0,90.000000000000,0,16,0,Steel - White Powder coated,Perforated steel,"Laminate, White, Matte",White Grille,"90Hz-17kHz ± 3dB, -10dB @ 65Hz",Wall bracket included,Black or white,"ABS, UL 94V-0 rated","LF: 5.25” /1” high-temp voice coil, coated paper, cone, rubber surround, ferrite motor, pressed steel chassis, HF: 0.75” silk dome, neodymium motor","(W) 152mm x (H) 245mm x (D) 140mm, (W) 6in x (H) 9.6in x (D) 5.5in",110° H x 80° V,75,Ultra-Compact Two-Way On-Wall System - Transformer,4.000000000000,12.000000000000,3.5 kHz passive (LF and HF auto-resetting fuses),Push terminals,"Rubber, Natural",0.260416666667,0,0.000000000000,90.000000000000,0,0,White Powder Coated Finish,90.000000000000,0.000000000000,D5030100,Waterproof connector cover,0,0,1,0,1,0,0,0,0.000000000000,0,0,0.000000000000,7.5,0,0,0,5,0
A80T - Black,20.02,https://martin-audio.com/,"Compact passive two-way system, front ported bass reflex",Steel - Black Powder coated,"70V: 60/30/15/7.5W, 100V: 60/30/15W",91,120,0.000000000000,7.5,"40Hz 24dB/oct (8 ohm), 60Hz 24dB/oct (Transformer)",VIA2502 or VIA5004 (or VIA5002 for70V/100V line),"200W AES, 800W peak",3.362239,https://martin-audio.com/products/loudspeakers/a80t,https://martin-audio.com/downloads/datasheets/ADORN-A80T-datasheet.pdf,90.000000000000,0.000000000000,10,A80T - Black,Martin Audio,0,0,90.000000000000,0,8,0,Steel - Black Powder coated,Perforated steel,"Laminate, Black, Matte",Black Grille,"63Hz-17kHz ± 3dB, -10dB @ 50Hz",6 x M6 inserts for wall or ceiling brackets,Black or white,"ABS, UL 94V-0 rated","LF: 8” with 2” high-temp voice coil, ferrite motor system, HF: 1” with 1” exit polymer dome compression driver","(W) 246mm x (H) 421mm x (D) 233mm, (W) 9.69in x (H) 16.56in x (D) 9.18in",90° H x 50° V,75,Ultra-Compact Two-Way On-Wall System - Transformer,4.000000000000,12.000000000000,2.3kHz passive (LF and HF auto-resetting fuses),Low profile 13A push-lock,"Rubber, Natural",0.437500000000,0,0.000000000000,90.000000000000,0,0,Black Finish,90.000000000000,0.000000000000,D5030100,IP54 rating with optional waterproof connector cover. Wall bracket WB6/8 (included),0,1,0,0,0,0,0,0,0.000000000000,0,0,0.000000000000,7.5,0,0,0,5,0
A80T - White,20.02,https://martin-audio.com/,"Compact passive two-way system, front ported bass reflex",Steel - White Powder coated,"70V: 60/30/15/7.5W, 100V: 60/30/15W",91,120,0.000000000000,7.5,"40Hz 24dB/oct (8 ohm), 60Hz 24dB/oct (Transformer)",VIA2502 or VIA5004 (or VIA5002 for70V/100V line),"200W AES, 800W peak",1.494328,https://martin-audio.com/products/loudspeakers/a80t,https://martin-audio.com/downloads/datasheets/ADORN-A80T-datasheet.pdf,90.000000000000,0.000000000000,10,A80T - White,Martin Audio,0,0,90.000000000000,0,8,0,Steel - White Powder coated,Perforated steel,"Laminate, White, Matte",White Grille,"63Hz-17kHz ± 3dB, -10dB @ 50Hz",6 x M6 inserts for wall or ceiling brackets,Black or white,"ABS, UL 94V-0 rated","LF: 8” with 2” high-temp voice coil, ferrite motor system, HF: 1” with 1” exit polymer dome compression driver","(W) 246mm x (H) 421mm x (D) 233mm, (W) 9.69in x (H) 16.56in x (D) 9.18in",90° H x 50° V,75,Ultra-Compact Two-Way On-Wall System - Transformer,4.000000000000,8.000000000000,2.3kHz passive (LF and HF auto-resetting fuses),Low profile 13A push-lock,"Rubber, Natural",0.437500000000,0,0.000000000000,90.000000000000,0,0,Wear Resistant Textured White,90.000000000000,0.000000000000,D5030100,IP54 rating with optional waterproof connector cover. Wall bracket WB6/8 (included),1,0,0,0,0,0,0,0,0.000000000000,0,0,0.000000000000,7.5,0,0,0,2.5,0
