,White##OTHER##,Weight (lbs)##OTHER##,Weight (kg)##OTHER##,User Specifed Custom Color##OTHER##,Trim##OTHER##,Sensitivity##OTHER##,SX218GRID White##OTHER##,SX218GRID Black##OTHER##,SX218FKIT White##OTHER##,SX218FKIT Black##OTHER##,SX218##OTHER##,215 WHEELKIT##OTHER##,SX215##OTHER##,SX212##OTHER##,SX210##OTHER##,SX118##OTHER##,SX115##OTHER##,SX112##OTHER##,SX110##OTHER##,SPL Max##OTHER##,Rotation Offset##ANGLE##DECIMAL DEGREES,Rotation##ANGLE##DECIMAL DEGREES,Recommended Amplifier##OTHER##,Rated Power##OTHER##,Protective Grille##OTHER##,Product Page URL##OTHER##,Product Documentation Link##OTHER##,Pitch Offset##ANGLE##DECIMAL DEGREES,Pitch##ANGLE##DECIMAL DEGREES,Model##OTHER##,Manufacturer##OTHER##,Add WHEELKIT##OTHER##,Include Feet##OTHER##,Impedance##OTHER##,Hardware Finish##OTHER##,Grill Scrim##OTHER##,Grill Finish##OTHER##,Frequency Response##OTHER##,Fittings##OTHER##,Finish##OTHER##,Enclosure##OTHER##,Driver##OTHER##,Dimensions (incl feet)##OTHER##,Dispersion (-6dB)##OTHER##,Description##OTHER##,Crossover##OTHER##,Connectors##OTHER##,Case Finish##OTHER##,Black##OTHER##,Azimuth Offset##ANGLE##DECIMAL DEGREES,Azimuth##ANGLE##DECIMAL DEGREES,Add WRKIT##OTHER##,Add SX218GRID##OTHER##,Add SF218FKIT##OTHER##,Accessories##OTHER##,218 WRKIT##OTHER##,218 WHEELKIT##OTHER##,215 WRKIT##OTHER##,118 WRKIT##OTHER##,118 WHEELKIT##OTHER##,115 WRKIT##OTHER##,115 WHEELKIT##OTHER##
SX110-W,1,26.5,12,N/A,"Plastic, Opaque White",97,0,0,0,0,0,0,0,0,0,0,0,0,1,121,90.000000000000,0.000000000000,VIA2502,250,Perforated steel,https://martin-audio.com/products/subwoofers/sx110,https://martin-audio.com/downloads/datasheets/SX110datasheet.pdf,-90.000000000000,0.000000000000,SX110-W,Martin Audio Ltd,0,1,8,Steel - White Powder coated,Grille Scrim - White,White Grille,50Hz-150Hz ± 3dB,12 x M8 inserts,White,Plywood,"1 x 10” (250mm)/2” (50mm) voice coil, long excursion, ferrite magnet",(W) 417mm x (H) 297mm x (D) 415mm. (W) 16.4ins x (H) 11.7ins x (D) 16.3ins,Omnidirectional,"Slimline, 10"" direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX110,0,26.5,12,N/A,"Plastic, Opaque Black",97,0,0,0,0,0,0,0,0,0,0,0,0,1,121,90.000000000000,0.000000000000,VIA2502,250,Perforated steel,https://martin-audio.com/products/subwoofers/sx110,https://martin-audio.com/downloads/datasheets/SX110datasheet.pdf,-90.000000000000,0.000000000000,SX110,Martin Audio Ltd,0,1,8,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,50Hz-150Hz ± 3dB,12 x M8 inserts,Black,,"1 x 10” (250mm)/2” (50mm) voice coil, long excursion, ferrite magnet",(W) 417mm x (H) 297mm x (D) 415mm. (W) 16.4ins x (H) 11.7ins x (D) 16.3ins,Omnidirectional,"Slimline, 10"" direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX110-RAL,0,26.5,12,Enter user specified RAL color,"Plastic, Opaque Black",97,0,0,0,0,0,0,0,0,0,0,0,0,1,121,90.000000000000,0.000000000000,VIA2502,250,Perforated steel,https://martin-audio.com/products/subwoofers/sx110,https://martin-audio.com/downloads/datasheets/SX110datasheet.pdf,-90.000000000000,0.000000000000,SX110-RAL,Martin Audio Ltd,0,1,8,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,50Hz-150Hz ± 3dB,12 x M8 inserts,User specified,,"1 x 10” (250mm)/2” (50mm) voice coil, long excursion, ferrite magnet",(W) 417mm x (H) 297mm x (D) 415mm. (W) 16.4ins x (H) 11.7ins x (D) 16.3ins,Omnidirectional,"Slimline, 10"" direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX112,0,47.3,21.5,N/A,"Plastic, Opaque Black",100,0,0,0,0,0,0,0,0,0,0,0,1,0,126,90.000000000000,0.000000000000,iK81 / VIA2502/5002/5004,400,Perforated steel,https://martin-audio.com/products/subwoofers/sx112,https://martin-audio.com/downloads/datasheets/SX112datasheet.pdf,-90.000000000000,0.000000000000,SX112,Martin Audio Ltd,0,1,8,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"48Hz-150Hz ± 3dB, -10dB @ 35Hz",12 x M10 inserts,Black,"52 litres, Plywood","12” (300mm)/3” (75mm) voice coil, long excursion, ferrite magnet, waterproof cone",(W) 487mm x (H) 390mm x (D) 410mm.  (W) 19.2ins x (H) 15.4ins x (D) 16.1ins,Omnidirectional,"Ultra-Compact, single 12"" driver, direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX115,0,80.5,36.5,N/A,"Plastic, Opaque Black",100,0,0,0,0,0,0,0,0,0,0,1,0,0,130,90.000000000000,0.000000000000,iK81 / VIA2502/5002/5004,1000,Perforated steel,https://martin-audio.com/products/subwoofers/sx115,https://martin-audio.com/downloads/datasheets/SX115datasheet.pdf,-90.000000000000,0.000000000000,SX115,Martin Audio Ltd,0,1,8,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"45Hz - 100Hz ± 3dB, -10dB @ 36Hz",24 x M10 inserts,Black,,"LF: 15” with 4” Voice coil, Ferrite Motor","(W) 500mm, (H) 451mm, (D) 678mm (806mm with Casters). (W) 19.69ins, (H) 17.76ins, (D) 26.69ins (31.73ins with Casters)",Omni-Directional/ or Cardioid (paired),15"" direct radiating subwoofer,100Hz,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX115W,1,80.5,36.5,N/A,"Plastic, Opaque White",100,0,0,0,0,0,0,0,0,0,0,1,0,0,130,90.000000000000,0.000000000000,iK81 / VIA2502/5002/5004,1000,Perforated steel,https://martin-audio.com/products/subwoofers/sx115,https://martin-audio.com/downloads/datasheets/SX115datasheet.pdf,-90.000000000000,0.000000000000,SX115-W,Martin Audio Ltd,0,1,8,Steel - White Powder coated,Grille Scrim - White,White Grille,"45Hz - 100Hz ± 3dB, -10dB @ 36Hz",24 x M10 inserts,White,,"LF: 15” with 4” Voice coil, Ferrite Motor","(W) 500mm, (H) 451mm, (D) 678mm (806mm with Casters). (W) 19.69ins, (H) 17.76ins, (D) 26.69ins (31.73ins with Casters)",Omni-Directional/ or Cardioid (paired),15"" direct radiating subwoofer,100Hz,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX118-W,1,96,43.5,N/A,"Plastic, Opaque White",102,0,0,0,0,0,0,0,0,0,1,0,0,0,138,90.000000000000,0.000000000000,"iKON iK42, iK81","1000W AES, 4000W peak",Black perforated Zintec,https://martin-audio.com/products/subwoofers/sx118,https://martin-audio.com/downloads/datasheets/SX118datasheet.pdf,-90.000000000000,0.000000000000,SX118-W,Martin Audio Ltd,0,1,8,Steel - White Powder coated,Grille Scrim - White,White Grille,"47Hz – 150Hz ±3dB, -10dB @ 41Hz","Two skids on base, with mating channels on top
M20 top-mounted thread plate for pole mounting
16 x M10 mounting points
2 x bar handles, 1 on each side
4 x fittings for optional transit cover
16 x M8 inserts for optional castors",Textured black paint,Multi-laminate birch/poplar ply,"18” (460mm)/4” (100mm) voice coil, long excursion, ferrite magnet, waterproof cone","(W) 600mm x (H) 509mm x (D) 632mm (760mm incl. castors), (W) 24in x (H) 20.36in x (D) 25.26in (30.38in incl. castors)",Omni-Directional/ or Cardioid (paired),18"" direct radiating subwoofer,,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX210-RAL,0,44.1,20,Enter specified RAL color....,"Plastic, Opaque Black",103,0,0,0,0,0,0,0,0,1,0,0,0,0,127,90.000000000000,0.000000000000,VIA2502/5002/5004,"500W AES, 2000W peak",Black perforated steel,https://martin-audio.com/products/subwoofers/sx210,https://martin-audio.com/downloads/datasheets/SX210datasheet.pdf,-90.000000000000,0.000000000000,SX210-RAL,Martin Audio Ltd,0,1,4,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"50Hz-150Hz ± 3dB, -10dB @ 42Hz","16 x M8 inserts, 2 x bar handles",User specified RAL color,Birch/poplar ply,"2 x 10” (250mm)/2” (50mm) voice coil, long excursion, ferrite magnet",(W) 718mm x (H) 295mm x (D) 465mm. (W) 28.3ins x (H) 11.4ins x (D) 18.3ins,Omnidirectional,"Slimline, dual 10"" direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX212,0,86,39,N/A,"Plastic, Opaque Black",106,0,0,0,0,0,0,0,1,0,0,0,0,0,132,90.000000000000,0.000000000000,iK42 / VIA5002/5004,"800W AES, 3200W peak",Black perforated steel,https://martin-audio.com/products/subwoofers/sx212,https://martin-audio.com/downloads/datasheets/SX212datasheet.pdf,-90.000000000000,0.000000000000,SX212,Martin Audio Ltd,0,1,4,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"48Hz-150Hz ± 3dB, -10dB @ 35Hz",12 x M10 inserts,Black textured paint,"100 litres, Plywood","2 x 12” (300mm)/3” (75mm) voice coil, long excursion, ferrite magnet, waterproof cone","(W) 872mm x (H) 390mm x (D) 437mm, (W) 34.3ins x (H) 15.4ins x (D) 17.2ins",Omnidirectional,"Compact, dual-12"" driver, direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX212-W,1,86,39,N/A,"Plastic, Opaque White",106,0,0,0,0,0,0,0,1,0,0,0,0,0,132,90.000000000000,0.000000000000,iK42 / VIA5002/5004,"800W AES, 3200W peak",White perforated steel,https://martin-audio.com/products/subwoofers/sx212,https://martin-audio.com/downloads/datasheets/SX212datasheet.pdf,-90.000000000000,0.000000000000,SX212-W,Martin Audio Ltd,0,1,4,Steel - White Powder coated,Grille Scrim - White,White Grille,"48Hz-150Hz ± 3dB, -10dB @ 35Hz",12 x M10 inserts,White textured paint,"100 litres, Plywood","2 x 12” (300mm)/3” (75mm) voice coil, long excursion, ferrite magnet, waterproof cone","(W) 872mm x (H) 390mm x (D) 437mm, (W) 34.3ins x (H) 15.4ins x (D) 17.2ins",Omnidirectional,"Compact, dual-12"" driver, direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX215,0,141,64,N/A,"Plastic, Opaque Black",103,0,0,0,0,0,0,1,0,0,0,0,0,0,136,90.000000000000,0.000000000000,,2000,,https://martin-audio.com/products/subwoofers/sx215,https://martin-audio.com/downloads/datasheets/SX215datasheet.pdf,-90.000000000000,0.000000000000,SX215,Martin Audio Ltd,0,1,4,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"45Hz - 100Hz ± 3dB, -10dB @ 36Hz",18 x M10 inserts,Black,,"LF: 15” with 4” Voice coil, Ferrite Motor","(W) 961mm, (H) 463mm, (D) 679mm (807mm with Casters). (W) 37.83ins, (H) 18.23ins, (D) 26.73ins (31.77ins with Casters)",Omni-Directional/ or Cardioid (paired),"Dual 15"" Driver, Direct radiating subwoofer",100Hz,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX215-W,1,141,64,N/A,"Plastic, Opaque White",103,0,0,0,0,0,0,1,0,0,0,0,0,0,136,90.000000000000,0.000000000000,,2000,,https://martin-audio.com/products/subwoofers/sx215,https://martin-audio.com/downloads/datasheets/SX215datasheet.pdf,-90.000000000000,0.000000000000,SX215-W,Martin Audio Ltd,0,1,4,Steel - White Powder coated,Grille Scrim - White,White Grille,"45Hz - 100Hz ± 3dB, -10dB @ 36Hz",18 x M10 inserts,White,,"LF: 15” with 4” Voice coil, Ferrite Motor","(W) 961mm, (H) 463mm, (D) 679mm (807mm with Casters). (W) 37.83ins, (H) 18.23ins, (D) 26.73ins (31.77ins with Casters)",Omni-Directional/ or Cardioid (paired),"Dual 15"" Driver, Direct radiating subwoofer",100Hz,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX210-W,1,44.1,20,N/A,"Plastic, Opaque White",103,0,0,0,0,0,0,0,0,1,0,0,0,0,127,90.000000000000,0.000000000000,VIA2502/5002/5004,"500W AES, 2000W peak",White perforated steel,https://martin-audio.com/products/subwoofers/sx210,https://martin-audio.com/downloads/datasheets/SX210datasheet.pdf,-90.000000000000,0.000000000000,SX210-W,Martin Audio Ltd,0,1,4,Steel - White Powder coated,Grille Scrim - White,White Grille,"50Hz-150Hz ± 3dB, -10dB @ 42Hz","16 x M8 inserts, 2 x bar handles",White textured paint,Birch/poplar ply,"2 x 10” (250mm)/2” (50mm) voice coil, long excursion, ferrite magnet",(W) 718mm x (H) 295mm x (D) 465mm. (W) 28.3ins x (H) 11.4ins x (D) 18.3ins,Omnidirectional,"Slimline, dual 10"" direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX112-RAL,0,47.3,21.5,Enter specified RAL color.....,"Plastic, Opaque Black",100,0,0,0,0,0,0,0,0,0,0,0,1,0,126,90.000000000000,0.000000000000,iK81 / VIA2502/5002/5004,400,Perforated steel,https://martin-audio.com/products/subwoofers/sx112,https://martin-audio.com/downloads/datasheets/SX112datasheet.pdf,-90.000000000000,0.000000000000,SX112,Martin Audio Ltd,0,1,8,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"48Hz-150Hz ± 3dB, -10dB @ 35Hz",12 x M10 inserts,User specified RAL color,"52 litres, Plywood","12” (300mm)/3” (75mm) voice coil, long excursion, ferrite magnet, waterproof cone",(W) 487mm x (H) 390mm x (D) 410mm.  (W) 19.2ins x (H) 15.4ins x (D) 16.1ins,Omnidirectional,"Ultra-Compact, single 12"" driver, direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX112-W,1,47.3,21.5,N/A,"Plastic, Opaque White",100,0,0,0,0,0,0,0,0,0,0,0,1,0,126,90.000000000000,0.000000000000,iK81 / VIA2502/5002/5004,400,Perforated steel,https://martin-audio.com/products/subwoofers/sx112,https://martin-audio.com/downloads/datasheets/SX112datasheet.pdf,-90.000000000000,0.000000000000,SX112-W,Martin Audio Ltd,0,1,8,Steel - White Powder coated,Grille Scrim - White,White Grille,"48Hz-150Hz ± 3dB, -10dB @ 35Hz",12 x M10 inserts,White,"52 litres, Plywood","12” (300mm)/3” (75mm) voice coil, long excursion, ferrite magnet, waterproof cone",(W) 487mm x (H) 390mm x (D) 410mm.  (W) 19.2ins x (H) 15.4ins x (D) 16.1ins,Omnidirectional,"Ultra-Compact, single 12"" driver, direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX112-B-MAR,0,47.3,21.5,N/A,"Plastic, Opaque Black",100,0,0,0,0,0,0,0,0,0,0,0,1,0,126,90.000000000000,0.000000000000,iK81 / VIA2502/5002/5004,400,Perforated steel,https://martin-audio.com/products/subwoofers/sx112,https://martin-audio.com/downloads/datasheets/SX112datasheet.pdf,-90.000000000000,0.000000000000,SX112-B-MAR,Martin Audio Ltd,0,1,8,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"48Hz-150Hz ± 3dB, -10dB @ 35Hz",12 x M10 inserts,Marine Grade Finish,"52 litres, Plywood","12” (300mm)/3” (75mm) voice coil, long excursion, ferrite magnet, waterproof cone",(W) 487mm x (H) 390mm x (D) 410mm.  (W) 19.2ins x (H) 15.4ins x (D) 16.1ins,Omnidirectional,"Ultra-Compact, single 12"" driver, direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX112-W-MAR,1,47.3,21.5,N/A,"Plastic, Opaque White",100,0,0,0,0,0,0,0,0,0,0,0,1,0,126,90.000000000000,0.000000000000,iK81 / VIA2502/5002/5004,400,Perforated steel,https://martin-audio.com/products/subwoofers/sx112,https://martin-audio.com/downloads/datasheets/SX112datasheet.pdf,-90.000000000000,0.000000000000,SX112-B-MAR,Martin Audio Ltd,0,1,8,Steel - White Powder coated,Grille Scrim - White,White Grille,"48Hz-150Hz ± 3dB, -10dB @ 35Hz",12 x M10 inserts,Marine Grade Finish,"52 litres, Plywood","12” (300mm)/3” (75mm) voice coil, long excursion, ferrite magnet, waterproof cone",(W) 487mm x (H) 390mm x (D) 410mm.  (W) 19.2ins x (H) 15.4ins x (D) 16.1ins,Omnidirectional,"Ultra-Compact, single 12"" driver, direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX212-RAL,1,86,39,Enter specified RAL Color,"Plastic, Opaque White",106,0,0,0,0,0,0,0,1,0,0,0,0,0,132,90.000000000000,0.000000000000,iK42 / VIA5002/5004,"800W AES, 3200W peak",Perforated steel,https://martin-audio.com/products/subwoofers/sx212,https://martin-audio.com/downloads/datasheets/SX212datasheet.pdf,-90.000000000000,0.000000000000,SX212-RAL,Martin Audio Ltd,0,1,4,Steel - White Powder coated,Grille Scrim - White,White Grille,"48Hz-150Hz ± 3dB, -10dB @ 35Hz",12 x M10 inserts,User specified RAL color,"100 litres, Plywood","2 x 12” (300mm)/3” (75mm) voice coil, long excursion, ferrite magnet, waterproof cone","(W) 872mm x (H) 390mm x (D) 437mm, (W) 34.3ins x (H) 15.4ins x (D) 17.2ins",Omnidirectional,"Compact, dual-12"" driver, direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
SX118,0,96,43.5,N/A,"Plastic, Opaque Black",102,0,0,0,0,0,0,0,0,0,1,0,0,0,138,90.000000000000,0.000000000000,"iKON iK42, iK81",1000,Black perforated Zintec,https://martin-audio.com/products/subwoofers/sx118,https://martin-audio.com/downloads/datasheets/SX118datasheet.pdf,-90.000000000000,0.000000000000,SX118,Martin Audio Ltd,0,1,8,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"47Hz – 150Hz ±3dB, -10dB @ 41Hz","Two skids on base, with mating channels on top
M20 top-mounted thread plate for pole mounting
16 x M10 mounting points
2 x bar handles, 1 on each side
4 x fittings for optional transit cover
16 x M8 inserts for optional castors",Black,Multi-laminate birch/poplar ply,"18” (460mm)/4” (100mm) voice coil, long excursion, ferrite magnet, waterproof cone","(W) 600mm x (H) 509mm x (D) 632mm (760mm incl. castors), (W) 24in x (H) 20.36in x (D) 25.26in (30.38in incl. castors)",Omni-Directional/ or Cardioid (paired),Compact 18"" Direct radiating subwoofer,100Hz,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,"16 x M8 inserts for optional castors, Input Board Cover, Transit Cover",0,0,0,0,0,0,0
SX118-B-MAR,0,96,43.5,N/A,"Plastic, Opaque Black",102,0,0,0,0,0,0,0,0,0,1,0,0,0,138,90.000000000000,0.000000000000,"iKON iK42, iK81",1000,Black perforated Zintec,https://martin-audio.com/products/subwoofers/sx118,https://martin-audio.com/downloads/datasheets/SX118datasheet.pdf,-90.000000000000,0.000000000000,SX118-B-MAR,Martin Audio Ltd,0,1,8,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"47Hz – 150Hz ±3dB, -10dB @ 41Hz","Two skids on base, with mating channels on top
M20 top-mounted thread plate for pole mounting
16 x M10 mounting points
2 x bar handles, 1 on each side
4 x fittings for optional transit cover
16 x M8 inserts for optional castors",Black Marine Grade Finish,Multi-laminate birch/poplar ply,"18” (460mm)/4” (100mm) voice coil, long excursion, ferrite magnet, waterproof cone","(W) 600mm x (H) 509mm x (D) 632mm (760mm incl. castors), (W) 24in x (H) 20.36in x (D) 25.26in (30.38in incl. castors)",Omni-Directional/ or Cardioid (paired),Compact 18"" Direct radiating subwoofer,100Hz,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,"16 x M8 inserts for optional castors, Input Board Cover, Transit Cover",0,0,0,0,0,0,0
SX118-W-MAR,1,96,43.5,N/A,"Plastic, Opaque White",102,0,0,0,0,0,0,0,0,0,1,0,0,0,138,90.000000000000,0.000000000000,"iKON iK42, iK81",1000,Black perforated Zintec,https://martin-audio.com/products/subwoofers/sx118,https://martin-audio.com/downloads/datasheets/SX118datasheet.pdf,-90.000000000000,0.000000000000,SX118-W-MAR,Martin Audio Ltd,0,1,8,Steel - White Powder coated,Grille Scrim - White,White Grille,"47Hz – 150Hz ±3dB, -10dB @ 41Hz","Two skids on base, with mating channels on top
M20 top-mounted thread plate for pole mounting
16 x M10 mounting points
2 x bar handles, 1 on each side
4 x fittings for optional transit cover
16 x M8 inserts for optional castors",Black Marine Grade Finish,Multi-laminate birch/poplar ply,"18” (460mm)/4” (100mm) voice coil, long excursion, ferrite magnet, waterproof cone","(W) 600mm x (H) 509mm x (D) 632mm (760mm incl. castors), (W) 24in x (H) 20.36in x (D) 25.26in (30.38in incl. castors)",Omni-Directional/ or Cardioid (paired),Compact 18"" Direct radiating subwoofer,100Hz,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,"16 x M8 inserts for optional castors, Input Board Cover, Transit Cover",0,0,0,0,0,0,0
SX218,0,217,95.5,N/A,"Plastic, Opaque Black",105,0,0,0,0,1,0,0,0,0,0,0,0,0,144,90.000000000000,0.000000000000,iKON iK42,2000,Perforated Zintec,https://martin-audio.com/products/subwoofers/sx218,https://martin-audio.com/downloads/datasheets/SX218datasheet.pdf,-90.000000000000,0.000000000000,SX218,Martin Audio Ltd,0,1,4,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"35Hz – 150Hz ±3dB, -10dB @ 30Hz","Two skids on base, with mating channels on top
24 x M10 mounting points
4 x bar handles, 2 on each side
4 x fittings for optional transit cover
M20 Pole mount insert
16 x M8 inserts for optional castors",Black textured paint,Multi-laminate birch/poplar ply,"2 x 18” (460mm)/4” (100mm) voice coil, long excursion, ferrite magnet, waterproof cone","((W) 1093mm x (H) 537mm x (D) 792mm 
 (920mm including castors). (W) 43in x (H) 21.1in x (D) 31.2in (36.2in including castors)",Omni-Directional/ or Cardioid (paired),"Dual 18"" Driver, Direct radiating subwoofer",100Hz,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,"16 x M8 inserts for optional castors, Input Board Cover, Transit Cover",0,0,0,0,0,0,0
SX218-W,1,217,95.5,N/A,"Plastic, Opaque White",105,0,0,0,0,1,0,0,0,0,0,0,0,0,144,90.000000000000,0.000000000000,iKON iK42,2000,Perforated Zintec,https://martin-audio.com/products/subwoofers/sx218,https://martin-audio.com/downloads/datasheets/SX218datasheet.pdf,-90.000000000000,0.000000000000,SX218-W,Martin Audio Ltd,0,1,4,Steel - White Powder coated,Grille Scrim - White,White Grille,"35Hz – 150Hz ±3dB, -10dB @ 30Hz","Two skids on base, with mating channels on top
24 x M10 mounting points
4 x bar handles, 2 on each side
4 x fittings for optional transit cover
M20 Pole mount insert
16 x M8 inserts for optional castors",White textured paint,Multi-laminate birch/poplar ply,"2 x 18” (460mm)/4” (100mm) voice coil, long excursion, ferrite magnet, waterproof cone","(W) 109mm x (H) 537mm x (D) 792mm 
 (920mm including castors). (W) 43in x (H) 21.1in x (D) 31.2in (36.2in including castors)",Omni-Directional/ or Cardioid (paired),"Dual 18"" Driver, Direct radiating subwoofer",100Hz,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,"16 x M8 inserts for optional castors, Input Board Cover, Transit Cover",0,0,0,0,0,0,0
SX218-W-MAR,1,217,95.5,N/A,"Plastic, Opaque White",105,0,0,0,0,1,0,0,0,0,0,0,0,0,144,90.000000000000,0.000000000000,iKON iK42,2000,Perforated Zintec,https://martin-audio.com/products/subwoofers/sx218,https://martin-audio.com/downloads/datasheets/SX218datasheet.pdf,-90.000000000000,0.000000000000,SX218-W-MAR,Martin Audio Ltd,0,1,4,Steel - White Powder coated,Grille Scrim - White,White Grille,"35Hz – 150Hz ±3dB, -10dB @ 30Hz","Two skids on base, with mating channels on top
24 x M10 mounting points
4 x bar handles, 2 on each side
4 x fittings for optional transit cover
M20 Pole mount insert
16 x M8 inserts for optional castors",White Marine Grade Finish,Multi-laminate birch/poplar ply,"2 x 18” (460mm)/4” (100mm) voice coil, long excursion, ferrite magnet, waterproof cone","((W) 1093mm x (H) 537mm x (D) 792mm 
 (920mm including castors). (W) 43in x (H) 21.1in x (D) 31.2in (36.2in including castors)",Omni-Directional/ or Cardioid (paired),"Dual 18"" Driver, Direct radiating subwoofer",100Hz,2 x NL4 type,Wear Resistant Textured White,0,90.000000000000,0.000000000000,0,0,0,"16 x M8 inserts for optional castors, Input Board Cover, Transit Cover",0,0,0,0,0,0,0
SX218-B-MAR,0,217,95.5,N/A,"Plastic, Opaque Black",105,0,0,0,0,1,0,0,0,0,0,0,0,0,144,90.000000000000,0.000000000000,iKON iK42,2000,Perforated Zintec,https://martin-audio.com/products/subwoofers/sx218,https://martin-audio.com/downloads/datasheets/SX218datasheet.pdf,-90.000000000000,0.000000000000,SX218-B-MAR,Martin Audio Ltd,0,1,4,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"35Hz – 150Hz ±3dB, -10dB @ 30Hz","Two skids on base, with mating channels on top
24 x M10 mounting points
4 x bar handles, 2 on each side
4 x fittings for optional transit cover
M20 Pole mount insert
16 x M8 inserts for optional castors",Black Marine Grade Paint,Multi-laminate birch/poplar ply,"2 x 18” (460mm)/4” (100mm) voice coil, long excursion, ferrite magnet, waterproof cone","((W) 1093mm x (H) 537mm x (D) 792mm 
 (920mm including castors). (W) 43in x (H) 21.1in x (D) 31.2in (36.2in including castors)",Omni-Directional/ or Cardioid (paired),"Dual 18"" Driver, Direct radiating subwoofer",100Hz,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,"16 x M8 inserts for optional castors, Input Board Cover, Transit Cover",0,0,0,0,0,0,0
SX210,0,44.1,20,N/A,"Plastic, Opaque Black",103,0,0,0,0,0,0,0,0,1,0,0,0,0,127,90.000000000000,0.000000000000,VIA2502/5002/5004,"500W AES, 2000W peak",White perforated steel,https://martin-audio.com/products/subwoofers/sx210,https://martin-audio.com/downloads/datasheets/SX210datasheet.pdf,-90.000000000000,0.000000000000,SX210-W,Martin Audio Ltd,0,1,4,Steel - Black Powder coated,Grille Scrim - Black,Black Grille,"50Hz-150Hz ± 3dB, -10dB @ 42Hz","16 x M8 inserts, 2 x bar handles",White textured paint,Birch/poplar ply,"2 x 10” (250mm)/2” (50mm) voice coil, long excursion, ferrite magnet",(W) 718mm x (H) 295mm x (D) 465mm. (W) 28.3ins x (H) 11.4ins x (D) 18.3ins,Omnidirectional,"Slimline, dual 10"" direct radiating subwoofer",80-120Hz active,2 x NL4 type,Wear Resistant Textured Black Paint,1,90.000000000000,0.000000000000,0,0,0,,0,0,0,0,0,0,0
